# CWR - Torque Wrench

Torque wrench model CWR-85 has range 15-85 Nm.

Point and click on image to see more information:

1 | Disengagement pin Press and lift
2 | Direction switch Turn to change the direction of rotation
3 | 3/8" reversible head
4 | Lever arm Do not grip for tightening
5 | Tactile and audible "click" feedback

Important:

- Do not overshoot the click.

- Do not push hard to achieve torque. It can break the internal sensors of the tensioner.

- Hold from the grip, not from the lever arm.

- Keep it disengaged during transportation.

Fore more information about CWR-85, please visit https://servaid.atlascopco.com/AssertWeb/en-US/AtlasCopco/Catalogue/8658

## Applies to: