# Manual Mode

1. On the Tasks tab on the hand controller, select Manual mode, then set pressure in the Set Target Pressure. Accept to start the pump.

2. Start building pressure by pressing the pressurize button. Press and hold.

3. Tighten the nut while holding the pressurize button pressed until all LEDs are green and then release the pressurize button.

Use manual mode for tensioning in the following cases:

- To initially check if the system is working and building pressure. Do not perform the phase Check Cycle at higher than 200 bar pressure.

- De-tensioning the nut.

## Applies to: