# Transportation

## System components

System components come in one box which includes: batteries, battery nutrunner, click wrench, hoses and hand controller (PFHC).

Before sending tools onsite, check that the following is done:

- Batteries are charged

- Click wrench is set to 75 Nm

- Nutrunner is adjusted to max torque and medium speed.

## Tensioner

Tensioner is supplied as a kit with a frame installed in an individual box and it includes a pressure test and calibration certificates.

Keep the connector protection caps always connected when the tensioner is not in use.

## Hydraulic pump/power pack

The pump is supplied without oil and has two caps, red and black. The red cap should be used when the pump is in use, and when the pump is being transported use the black cap.

Make sure to use the right grade of oil as per ambient temperature. Only ISO VG oil with high viscosity index over 140 is permitted.

## Applies to: