# Assembling the Swivel Manifold

The Torcflex wrench can be fitted with 2 types of swivel manifold. Follow the instructions below to replace or change the manifold when needed.

Use Loctite 243 as thread locker to prevent loosening on assemblies.

Model | Hex Key (mm) | Torque (Nm)
--- | --- | ---
TFX02 | 4 | 11
TFX04–TFX30 | 5 | 18

## Installing a Co-axial Swivel Manifold

## Installing a Twin-line Swivel Manifold

## Applies to: