# Pressure Testing

1. Connect the wrench to the pump.

2. Press and release the Advance [1] button to start the pump. Wait for 10 seconds and look for any signs of oil leaks.

3. Press and hold the Advance button and pressurize the tool to 690 bar (10,000 psi). Hold for 10 seconds and look for any signs of oil leaks.

4. Release the button and pressurize again 3 times, look for any signs of oil leaks each time.

## Applies to: