# Connecting the Hose to the Pump

1. Hold the pump frame (1) to prevent the pump from moving during the connection. Position the hose nipple (2) in line with the pump coupling.

2. Firmly push the hose nipple and pump coupling together (2). A click is heard when the connection is complete.

   The knurled collar on the pump coupling does not need to be drawn back during the connection.

3. Pull the hose (3) to make sure that the connection is correct.

## Applies to: