# Connecting the Hose to the Wrench

1. Support the swivel manifold at the opposite side to the coupling (1). Position the hose coupling in line with the wrench nipple (2).

2. Firmly push the wrench nipple and hose coupling together. A click is heard when the connection is complete.

   The knurled collar on the hose coupling does not need to be drawn back during the connection.

3. Pull the hose (3) to make sure that the connection is correct.

## Applies to: