# Network Configurations

The tool can be set up to be accessed wirelessly from a web browser on a Local Area Network (LAN), using IPv4 protocol.

There is an option to use the tool as a client or an access point for other devices.

Preparations

1. Remove the cover of the tool's USB connection port.

2. Connect the tool to the USB-port of the PC.

3. Open a web browser and type in the address 169.254.1.1.

In this Section

- Configuring Bluetooth
- Configuring Channels
- Configuring a Wireless Client
- Configuring the Tool as a Wireless Access Point