# Logging on to Smart AMS Config

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

A dialog box will appear in the web browser prompting you to enter your username and password.

The first time you use Smart AMS Config, you are prompted to specify a username and password. You will then need to enter these credentials to log on to Smart AMS Config as a superuser.

- Enter your credentials to log on. You can get this information from the person responsible for Smart AMS configuration.

The data you enter in the Username and Password fields must match those of an existing user account.

## Applies to: