# Adding and managing stations

You must first navigate to Smart AMS Config.

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

- To switch to the Workplaces section, click in the Navigation Panel on the left of the page.

The number of bolts and the number of tightening equipment items assigned to a station will appear on the station icon in the Workplaces section.

- To add a station, click to the right of the line's name, and then select Smart AMS Station, SQS Station, or Manual Station. If the station does not have a connection to Smart AMS, select Manual Station; Smart AMS will be ignoring it.

- To rearrange stations in the line, use a drag-and-drop operation.

- To copy a station, to paste it, or delete it, use the right-click context menu of the station.

In this Section

- Specifying settings for Smart AMS station
- Adding and managing controllers at Smart AMS stations
- Adding a recipe
- Specifying settings for SQS3 station
- Specifying settings for manual station

## Applies to: