# Changing locale

You must first navigate to Smart AMS Manager.

- Go to the Smart AMS Manager address in your web browser by using the Open Smart AMS Manager shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6394. Port number is selected when you install Smart AMS. The default is 6394. Make sure to replace localhost with the actual IP address of the computer that Smart AMS Manager is running on.

- To switch to the Administration section, click in the Navigation Panel on the left of the page. On mobile devices with a smaller screen, click your username in the upper right corner of the page, and then select Administration.

- Click Profile.

- In the Locale list, select English, German, or Chinese.

For values shown in the Dashboard section, different locales use a decimal point or a comma, as appropriate.

## Applies to: