# Set-up Preparations

Prior to connecting the hydraulic pump to any bolt tensioning equipment, ensure that:

- The working pressure of the hydraulic pump and the equipment to be operated are compatible.

- The reservoir pump capacity is adequate to operate the equipment throughout its range.

- The hydraulic oil specification used within the pump and the equipment are compatible.

- The technical specifications of the tensioning tool is known.

Ensure sufficient stud protrudes above the hexagon or round joint nut.