# Seal Replacement “Clip - In” Type

Atlas Copco use different seal configurations due to differences in tensioner specifications and tensioner usage environments. This section details the replacement of Clip - In type high pressure seals.

No. | Description
--- | ---
1 | Seal Clip (outer)
2 | Seal Clip (inner)

1. Insert the inner seal into the seal housing. The seal clip fits into the seal clip housing.

2. With a blunt nose tool, push the seal fully into the seal clip housing. Work around the periphery of the seal until the seal is completely inserted into the clip housing.

3. Insert the outer seal into the seal housing. The seal clip fits into the seal clip housing.

4. With a blunt nose tool, push the seal fully into the seal clip housing. Work around the periphery of the seal until the seal is completely inserted into the clip housing.