# Hydraulic Nut System Configuration

The most efficient use of bolt tensioning tools is where every bolt is tensioned simultaneously; 100% bolt to tensioner ratio. Hydraulic nuts can be fitted to either one or both sides of the bolted joint depending on accessibility.

Generally with hydraulic nuts, 100% of the bolts are tensioned simultaneously.

Point and click on image to see more information:

1 | Link hose
2 | Link hose to the pump

Point and click on image to see more information:

1 | Link hose
2 | Link hose to the pump
3 | It is OK to leave a female coupler unconnected

## Hydraulic Nut Arrangement - 100% Configuration

On some applications, it is not possible to fit hydraulic nuts to every bolt from the same side of the bolted joint. In that case, it is necessary to stagger the hydraulic nuts over both sides of the bolted joint. In either configuration, it is normal practice to fit the bolts in such way so adequate thread protrudes from the side of the joint that the hydraulic nuts will be fitted. See the pictures below.

WARNING

Projectile Hazard

Never pressurize an unconnected male coupler. Male couplers are not designed to withstand high pressure, in the unconnected mode. Pressurizing an unconnected male coupler can lead to serious bodily injury or death.

- If you are left with an unconnected male connection, check the hydraulic hose assembly and correct the error.

It is safe to pressurize an unconnected female connection. The end, unconnected port on a chain of tensioners or hydraulic nuts should contain a female coupling or a blanking plug.

- Joint side A: Alternate stud bolts on a joint showing adequate stud bolt protrusion.

- Joint side B: Alternate studs on a joint showing adequate stud bolt protrusion.