# Top Collar Hydraulic Nut

## Hydraulic Nut

# Product Information

# General Information

WARNING

Risk of Property Damage or Severe Injury

Ensure that you read, understand and follow all instructions before operating the tool. Failure to follow all the instructions may result in electric shock, fire, property damage and/or severe bodily injury.

- Read all Safety Information delivered together with the different parts of the system.

- Read all Product Instructions for installation, operation and maintenance of the different parts of the system.

- Read all locally legislated safety regulations regarding the system and parts thereof.

- Save all Safety Information and instructions for future reference.

In this Section

- Safety Signal Words
- Warranty
- Website
- ServAid
- Safety Data Sheets MSDS/SDS
- Country of Origin
- Dimensional Drawings

# Safety Signal Words

The safety signal words Danger, Warning, Caution, and Notice have the following meanings:

DANGER | DANGER indicates a hazardous situation which, if not avoided, will result in death or serious injury.
WARNING | WARNING indicates a hazardous situation which, if not avoided, could result in death or serious injury.
CAUTION | CAUTION, used with the safety alert symbol, indicates a hazardous situation which, if not avoided, could result in minor or moderate injury.
NOTICE | NOTICE is used to address practices not related to personal injury.

# Warranty

- Product warranty will expire 12+1 months after dispatch from Atlas Copco's Distribution Center.

- Normal wear and tear on parts is not included within the warranty.

  - Normal wear and tear is that which requires a part change or other adjustment/overhaul during standard tools maintenance typical for that period (expressed in time, operation hours or otherwise).

- The product warranty relies on the correct use, maintenance, and repair of the tool and its component parts.

- Damage to parts that occurs as a result of inadequate maintenance or performed by parties other than Atlas Copco or their Certified Service Partners during the warranty period is not covered by the warranty.

- To avoid damage or destruction of tool parts, service the tool according to the recommended maintenance schedules and follow the correct instructions.

- Warranty repairs are only performed in Atlas Copco workshops or by Certified Service Partners.

Atlas Copco offers extended warranty and state of the art preventive maintenance through its ToolCover contracts. For further information contact your local Service representative.

For electrical motors:

- Warranty will only apply when the electric motor has not been opened.

# Website

Information concerning our Products, Accessories, Spare Parts and Published Matters can be found on the Atlas Copco website.

Please visit: www.atlascopco.com.

# ServAid

ServAid is a portal that is continuously updated and contains Technical Information, such as:

- Regulatory and Safety Information

- Technical Data

- Installation, Operation and Service Instructions

- Spare Parts Lists

- Accessories

- Dimensional Drawings

Please visit: https://servaid.atlascopco.com.

For further Technical Information, please contact your local Atlas Copco representative.

# Safety Data Sheets MSDS/SDS

The Safety Data Sheets describe the chemical products sold by Atlas Copco.

Please consult the Atlas Copco website for more information www.atlascopco.com/sds.

# Country of Origin

For the Country of Origin, please refer to the information on the product label.

# Dimensional Drawings

Dimensional Drawings can be found either in the Dimensional Drawings Archive, or on ServAid.

Please visit: http://webbox.atlascopco.com/webbox/dimdrw or https://servaid.atlascopco.com.

# Overview

# Technical Product Data

Technical Product Data can be found on either ServAid, or the Atlas Copco website.

Please visit: https://servaid.atlascopco.com or www.atlascopco.com.

# Installation

# Installation Instructions

# Hydraulic Nut Installation

## Preparations

- Read the section Hydraulic Nut System Configuration to select appropriate hydraulic nut arrangement.

- Make sure that the stud bolt threads are clean and free of damage.

## Installation

1. Use a tommy bar to make sure that the hydraulic nut is fully seated against the joint face.

2. The hydraulic nut is supplied fitted with blanking plugs in order to save space during packaging. Choose the most accessible port and remove the blanking plug.

3. Replace the removed blanking plug with a suitable high-pressure male coupling.

   Do not overtighten the connection, it can damage the male sealing cone.

   Hydraulic couplers of either type should be tightened into the tool from the adaptor piece only. Required tightening torque is 25Nm

4. Connect the hydraulic nut to a suitable Atlas Copco pump by a length of link hose. A link hose is a length of high-pressure hydraulic hose with a male coupling at one end and a female coupling at the other.

   If simultaneous tensioning of more than one bolt is to be carried out, fit one male and one female quick connect coupling to each hydraulic nut, and by using link hoses, link each nut together. The end nut on the application should have either an unconnected female coupling (to a link hose) or a blanking plug.

   For pump operation, refer to the supplied pump instruction document.

   Refer to the technical details that are hard stamped on the hydraulic nut.

   Make sure to have knowledge about the maximum operating pressure and maximum piston movement of the hydraulic nut.

   Be aware of the pressure needed to induce the required bolt load.

# Hydraulic Nut System Configuration

The most efficient use of bolt tensioning tools is where every bolt is tensioned simultaneously; 100% bolt to tensioner ratio. Hydraulic nuts can be fitted to either one or both sides of the bolted joint depending on accessibility.

Generally with hydraulic nuts, 100% of the bolts are tensioned simultaneously.

Point and click on image to see more information:

1 | Link hose
2 | Link hose to the pump

Point and click on image to see more information:

1 | Link hose
2 | Link hose to the pump
3 | It is OK to leave a female coupler unconnected

## Hydraulic Nut Arrangement - 100% Configuration

On some applications, it is not possible to fit hydraulic nuts to every bolt from the same side of the bolted joint. In that case, it is necessary to stagger the hydraulic nuts over both sides of the bolted joint. In either configuration, it is normal practice to fit the bolts in such way so adequate thread protrudes from the side of the joint that the hydraulic nuts will be fitted. See the pictures below.

WARNING

Projectile Hazard

Never pressurize an unconnected male coupler. Male couplers are not designed to withstand high pressure, in the unconnected mode. Pressurizing an unconnected male coupler can lead to serious bodily injury or death.

- If you are left with an unconnected male connection, check the hydraulic hose assembly and correct the error.

It is safe to pressurize an unconnected female connection. The end, unconnected port on a chain of tensioners or hydraulic nuts should contain a female coupling or a blanking plug.

- Joint side A: Alternate stud bolts on a joint showing adequate stud bolt protrusion.

- Joint side B: Alternate studs on a joint showing adequate stud bolt protrusion.

# Operation

# Operating Instructions

# Pre-Procedure Checks

Components

- Check that each bolt to be tensioned is visually free from obvious thread defects. Make sure that all hydraulic nuts are free to rotate on the bolts and can be wound flush up against the application face. Refer to the general arrangement drawing of your particular tensioner to confirm the correct level of the required bolt protrusion. Also, make sure that full thread engagement is available through the nut on the opposite end of the bolt being tensioned.

- Check that all calculations pertaining to the tensioning procedure, including pressures, bolt loads, etc are available and have been reviewed by a qualified engineer with bolting experience.

- Inspect the hose to make sure that no cracking, peeling or other damage has occurred to the polyamide material of the hose. Damaged hose must be replaced.

Pump

- Make sure that personnel has fully read and understood the Product Instructions and Safety Information for the pump.

- Make sure that the pump reservoir is filled with an adequate oil volume.

- Make sure that the correct and preferred grade of oil is used in the pump.

Personnel

- Make sure that all personnel are aware of the maximum working pressure and maximum piston stroke of the tensioners. These details are hard stamped on the tensioner body.

- Always make sure that all personnel in the near vicinity are aware that pressurization of high pressure equipment is about to take place. Cordon off the working area and exclude anyone from the area who is not involved directly with the tensioning procedure.

- Make sure that personnel are fully trained in stud bolt tensioning procedures and have fully read this guide and safety notes.

- Bolting calculations must be done by qualified engineers who are properly trained or have suitable experience in bolting technology.

# Maximum Stroke Indicator

The maximum approved stroke of the hydraulic nut is indicated by a red line hard stamped into the circumference of the piston.

Red piston overstroke indicator.
Red piston overstroke indicator.

Continually monitor the piston stroke during the tensioner pressurization. If the maximum piston stroke indicator becomes visible on any of the hydraulic nuts before the target pressure is reached, immediately stop the pump and release the pressure to zero. Rotate the hydraulic nut pistons until the pistons are shut down into the zero stroke position. Recommence the tensioning procedure.

Failure to stop the tensioning sequence once the red piston indicator becomes visible, can result in failure of the tensioner seal and will eventually cause a release of high pressure fluid which can lead to injury or death.

Escaping high-pressure oil can penetrate the skin and is extremely dangerous. Seek urgent medical attention if oil penetrates skin.

# Tensioning Procedure

WARNING

High-Pressure Fluids Hazard

Never grab, touch, or in any way come in contact with a hydraulic pressure leak. When the hydraulic circuit is pressurized, the hydraulic fluid can escape at high speed. Escaping fluid under pressure can penetrate the skin causing serious injury. If an accident occurs, contact the nearest health service immediately! Any fluid injected into the skin must be surgically removed within a few hours or gangrene may result.

- Always relieve pressure before disconnecting hydraulic or other lines. Tighten all connections before applying pressure.

- Always wear safety approved eye wear when checking for leaks. Do not use your hands to check for leaks in the hydraulic circuit.

- Always keep away from leaking elements during the tightening process.

- Always wear impact-resistant eye and face protection when involved with or near the operation, repair or maintenance of the unit.

- Be sure all others in the area are wearing impact-resistant eye and face protection.

- Even small projectiles can injure eyes and cause blindness.

WARNING

Risk of Severe Injury

Always use personal protective equipment when operating the unit. Below are possible hazardous situations:

- Impact blows to the head

- Foot injuries

- Exposure to high noise levels

- Heat, splashes from liquids, impacts, cuts, air contaminated with harmful dusts, fumes, mists, sprays, and vapors.

If not avoided, the above hazardous situations could result in severe bodily injury or death.

- Always use the adequate personal protective equipment on your job site.

WARNING

Risk of Severe Injury

Always protect the face when working with high-pressure equipment. High-pressure equipment could cause severe bodily injury.

- Always wear goggles and/or face shield.

- Monitor the pressurized equipment and pay attention to the pressure gauge, because the pressure can increase quite rapidly in case of low volume circuits.

WARNING

Projectile Hazard

Never pressurize an unconnected male coupler. Male couplers are not designed to withstand high pressure, in the unconnected mode. Pressurizing an unconnected male coupler can lead to serious bodily injury or death.

- If you are left with an unconnected male connection, check the hydraulic hose assembly and correct the error.

WARNING

Projectile Hazard

Unexpected bolt failure can result in serious personal injury or death. Premature bolt failure can lead to parts of the tensioner or bolt becoming high velocity projectiles.

- Never stand in-line with the bolt axis during the tensioning or de-tensioning procedure.

- Alert all personnel to the consequences of premature bolt failure and clear the area of non essential personnel before the procedure starts.

## Procedure

1. Make sure that the two halves of the bolted joint are fully and correctly aligned.

2. Fit the hydraulic nuts to all of the stud bolts.

   See section Hydraulic Nut System Configuration for configuration illustrations of hydraulic nut set up.

   See section Hydraulic Nut Installation for installation instructions.

3. Make sure the pump is turned off and the pressure release valve is in the open position.

4. By using suitable link hoses, connect the hydraulic nuts together and to a suitable pump unit.

   If simultaneous tensioning of more than one bolt is to be carried out, fit one male and one female quick connect coupling to each hydraulic nut, and by using link hoses, link each nut together. The end nut on the application should have either an unconnected female coupling (to a link hose) or a blanking plug.

   Make sure the tensioning team is aware of the target working pressure.

5. Operate the pump unit and pressurize the system 1000 psi (70 bar). Make sure that the pressure is holding steady. If the pressure drops, investigate the problem by looking for leaks. For pump operation, see the Product Instructions for the pump.

   Never exceed the maximum working pressure.

   Never leave high pressure hydraulic tools unattended while pressurized.

   The system must be at zero pressure before starting any investigation, maintenance or leak repair work.

   Maximum stroke is indicated with the red line above the threads on the piston.

   Never exceed the maximum piston stroke capability of the tensioning tool.

   If the maximum stroke indicator appears on any of the tools before the target operating pressure is reached, immediately stop the pressurization sequence. Slowly open the pump pressure release valve and make sure that the pressure drops to zero. Return the body and restart the tensioning procedure.

6. When the pressure is holding steady, continue to pressurize the system up to the target calculated working pressure.

7. When the required pressure is achieved, hold the pressure. To retain the bolt load, firmly tighten the load retaining collar down against the nut body, with the tommy bar and a mallet.

   In order to retain enough preload, the load collar must be firmly seated.

8. When the collar is seated properly down against the top face of the load cell body, the piston of the hydraulic nut is clearly visible above the collar.

9. Release the pump pressure.

10. Remove the hydraulic link hose from the hydraulic nut.

11. Unscrew and remove the hydraulic connection.

12. Replace the original blanking plug to prevent the ingress of contaminants into the internals of the hydraulic nut.

    Hydraulic couplers of either type must be tightened into the tool from the adaptor piece only. Required tightening torque is 25Nm.

# De-Tensioning Procedure

1. Choose the most accessible port and remove the blanking plug.

2. Replace the removed blanking plug with a male hydraulic fitting.

   Hydraulic couplers of either type should be tightened into the tool from the adaptor piece only. Required tightening torque is 25Nm.

   Do not overtighten the connection, it can damage the male sealing cone in the fitting.

   Bolting calculations must be done by qualified engineers who are properly trained or have suitable experience in bolting technology.

   If simultaneous tensioning of more than one bolt is to be carried out, fit one male and one female quick connect coupling to each hydraulic nut, and by using link hoses, link each nut together. The end nut on the application should have either an unconnected female coupling (to a link hose) or a blanking plug.

3. Connect the hydraulic nut to a suitable Atlas Copco pump unit by a length of link hose. A link hose is a length of high-pressure hydraulic hose with a male coupling at one end and a female coupling at the other.

   Make sure that the pressure rating for the Atlas Copco link hose matches the maximum working pressure of the tool. Refer to the hard stamped details on the hydraulic nut.

   The system must be at zero pressure before starting any investigation, maintenance or leak repair work.

   During the de-tensioning procedure NEVER exceed the maximum working pressure of the hydraulic nut.

   Definition: Break Loose Pressure (BLP) is the pressure at which the user can rotate the load retaining collar on the hydraulic nuts by hand with a tommy bar.

4. Once the pressure is holding steady, continue to slowly increase the pressure. Apply a light force to a tommy bar inserted into the collar. As soon as the collar rotates, BLP is reached. Once the BLP is found, stop the pump to hold the pressure and make a note of the pressure

   Never exceed the maximum working pressure.

5. While holding the pressure, rotate the load retaining collar up, away from the hydraulic nut body.

   Make sure that enough space is left below the collar for the piston to allow fully retract into the hydraulic nut body.

   If locking collars are difficult to rotate at this BLP, slightly increase the pressure until the locking dollar become loose.

   Never exceed the maximum working pressure of the hydraulic nuts.

   Make sure that the bolt material and joint material can withstand the load you are applying.

   In the example shown in the picture below, the collar is backed off until it is level with the top of the piston. Therefore it allows the piston to fully return into the body without re-applying the load to the collar.

   Never stand in line with the bolt axis while seating the collar. Unexpected bolt failure can result in serious personal injury or death.

6. Release the pressure from the pump. Remove the hydraulic link hose and hydraulic coupling from the hydraulic nut.

   Only attempt to uncouple high pressure hydraulics while the system is not holding any pressure.

   Never attempt to remove fittings from a high pressure hydraulic tool when the system is pressurized. Escaping high-pressure oil can penetrate the skin and is extremely dangerous. Seek urgent medical attention if oil penetrates skin.

7. Replace the blanking plug in the hydraulic nut to prevent the ingress of contaminations into the hydraulic nut during storage and transport.

8. Disassemble the hydraulic nut from the bolt. If the hydraulic nut cannot be disassembled, the collar was not wound back enough and there is still load trapped in the joint. Repeat the de-tensioning process from step 1.

# Service

# Seal Replacement “Clip - In” Type

Atlas Copco use different seal configurations due to differences in tensioner specifications and tensioner usage environments. This section details the replacement of Clip - In type high pressure seals.

No. | Description
--- | ---
1 | Seal Clip (outer)
2 | Seal Clip (inner)

1. Insert the inner seal into the seal housing. The seal clip fits into the seal clip housing.

2. With a blunt nose tool, push the seal fully into the seal clip housing. Work around the periphery of the seal until the seal is completely inserted into the clip housing.

3. Insert the outer seal into the seal housing. The seal clip fits into the seal clip housing.

4. With a blunt nose tool, push the seal fully into the seal clip housing. Work around the periphery of the seal until the seal is completely inserted into the clip housing.

# Seal Replacement S2/K2 Type

Atlas Copco use different seal configurations due to differences in tensioner specifications and tensioner usage environments. This section details the replacement of S2/K2 type high pressure seals.

1. Make note of the correct orientation of the triangular backup ring.

2. Put the outer backup ring into the piston outer seal housing.

3. Position and stretch the outer seal into the piston outer seal housing.

   The seal fits above the backup ring.

4. With a rounded smooth screwdriver, push the seal until the seal clips into the seal housing.

   Make sure that the seal and backup ring are fully seated around circumference.

5. Squeeze the inner seal into the inner seal housing.

6. Push the inner seal in place with a smooth rounded screwdriver.

7. Put the inner backup ring below the inner seal.

8. Carefully bend the backup ring to enable it to clip into position. Make sure that the seal and backup ring are fully seated around the circumference.

# Maintenance Instructions

# Service Recommendations

Preventive maintenance is recommended at regular intervals. See the detailed information on preventive maintenance. If the product is not working properly, take it out of service and inspect it.

If no detailed information about preventive maintenance is included, follow these general guidelines:

- Clean appropriate parts accurately

- Replace any defective or worn parts

# Service Recommendations

## General Maintenance

Service must be done by authorized workshops or qualified service technicians.

- Examine the tool regularly for signs of corrosion. If signs of corrosion are found, return the tool to the nearest Atlas Copco service center for refurbishment.

- Examine the tool coating regularly for signs of cracking or flaking. If any cracking or flaking are found, it is recommended to return the tool to the nearest Atlas Copco service center for advice.

- Check lifting eyes and straps on tools for any cracks, tears or other visible damage. Do not use lifting straps or eyebolts that are found to be damaged.

- Tools should not be dropped or hit. This can cause damage to the sealing surfaces of the tool which can result in tool failure during usage.

- It is recommended to fully refurbish tools every 12 months.

- For advice about the operational suitability of the tool, contact Atlas Copco service center.

## Tool Storage and Preservation

- When the tensioning operation is complete, wipe down all components and carefully remove any water from the tensioner surfaces.

- Wipe or spray all surfaces, including those that contain a screwthread, with a non-drying rust prohibitive oil.

- Make sure that the dust caps are correctly fitted on all hydraulic fittings. This will prevent foreign objects from getting into the fittings and fouling them.

- Store the tool in an upright position.

- Store the tool with the ram retracted.

- Store the tool in a dry environment.

# Troubleshooting

Problem | Possible cause | Solution
--- | --- | ---
Hydraulic fluid accumulated on or leaking from hydraulic fittings. System will neither build nor hold pressure. | Fitting or adaptors are loose. | Tighten to torque values stated in assembly and recycling instructions.
Cannot connect hydraulic fittings. | Hydraulic nuts contain small amount of residual hydraulic pressure. | Slowly loosen fittings on hydraulic nut and/or hose to release residual pressure.
Fittings are damaged or worn. | Replace fittings.
Hydraulic fluid leaking from piston. System will not build pressure. | Hydraulic seals are worn or damaged. | Replace hydraulic seals.
Hydraulic nut difficult to screw onto bolt. Snagging or locking. | Damage on hydraulic nut or bolt. | Examine internal and external screwthreads for signs of damage or foreign particles. Minor damage can be carefully filed smooth with a needle file. Clean internal and external screwthreads with a wire brush and then wipe with a solvent.
Dirty screwthreads on hydraulic nut or bolt.