# Running a quick programming

1. In the Toolbar, tap Quick Programming.

2. In the Select transducer dialog box, select the transducer to use.

   If no devices are connected to the STpalm, an Error message is displayed.

3. In the Select tool strategy dialog box, select the strategy to use.

4. In the Quick programming page, tap Play () to run the inspection.

On the upper-right corner of the Quick programming page, tap Save to save the configuration of the Tool and the inspection configured by the quick programming.

The configuration of the Tool and Inspection is editable.

## Applies to: