# Adding Tool check inspection(s) through the template file

1. Generate the Template file for inspections and save it on a PC (for more information, see Generating Tool check / Joint check template).

2. On the PC, open the file STpad_ToolInspectionImportFile.xlsm. The following is displayed:

3. Complete the file STpad_ToolInspectionImportFile.xlsm to define the necessary inspection(s).

   When all the mandatory fields are filled in, the Wrong field column becomes green.

   The file STpad_ToolInspectionImportFile.xlsm defines not only inspection(s), but also the linked tool(s). These are automatically imported on the device through the file STpad_ToolInspectionImportFile.stpad.

   Check the Excel option for the workbook calculation. Open a Excel file and click File > Options. On left side of the Excel options dialog box, select Formulas > Automatic option for the Calculation options section.

4. When the Wrong field column in correspondence of the new inspection(s) is green colored, click the blue button Sort and export to automatically generate the file STpad_ToolInspectionImportFile.stpad.

   The file STpad_ToollnspectionImportFile.stpad is automatically saved on the PC.

   Only the STpad_ToolInspectionImportFile.stpad can be correctly imported on the device (for more information about how to import inspections, see Import inspections).

5. Save the file STpad_ToolInspectionImportFile.xlsm.

6. Close the file STpad_ToolInspectionImportFile.xlsm.

7. Import the inspection(s) saved in the file STpad_ToolInspectionImportFile.stpad on the device (for more information about how to import routes, see Importing the inspection(s) on the device).

8. Click the Menu icon > Tools to check the import of the inspection(s) is correctly done.

## Applies to: