# Running a free Route

1. Connect the device to the necessary measuring device (for more information, see “Measuring devices”).

2. Tap the route name or the Run icon to run the route.

3. In the Edit Route page - Inspection category, tap Play in correspondence of the inspection to be run (for more information, see “Inspections”).

   If necessary, in the Edit Route page - General category, edit the route parameters according to customer needs (for more information, see “Editing a Route”).

   The status of all the inspections, except ISO 5393, can be: To do, Partial, OK, or NOK.

   The status of the inspections ISO 5393 can be: To do, Partial, or Completed.

## Applies to: