# Generating the template file for joint check inspections

1. On the left side of the Toolbar, tap the Menu icon () > Configuration > Import / Export > Templates > Template file for Joint check inspections.

2. To generate the template for the configuration of the joint check inspections, tap the Generate button.

   The template file is saved in the SDcard\Download folder on the device.

3. On the Information message, tap OK.

4. Connect the device to the PC via USB cable.

5. In the Autoplay dialog box, select Open the device to see the files> Internal shared storage > Download > . Then, copy the STpad_JointInspectionImportFile.xlsm file on the PC.

   The file now is ready to be completed with the tool check inspection(s) to import on the device.

## Applies to: