# Joints

The set of parameters that controls a test process is within a joint. This section describes how to setup the joint parameters necessary to do a test.
The device can store up to 20000 joints into its own memory.
Tap the Menu icon in the Home page. Then, select Joints.
The following is displayed:

A | Barcode button | B | Command button
C | Play button | D | List of Joint
E | Search button |  |

In each row, the following information about the Joint are shown:

- Name

- Torque range

When enabled by external software, the Barcode button () allows to scan a barcode to search the corresponding Joint inspection(s) on the measuring device. If the search finds a single Joint inspection, it is automatically run; if the search finds multiple Joint inspections with the same barcode identifier, run the inspection of interest from the list.

Play () gets active only after adding Inspection(s) to the Joint. If enabled, tap Play to run the test.

In this Section

- Adding a Joint
- Joint parameters
- Deleting a Joint
- Editing a Joint
- Searching a Joint

## Applies to: