# Joint inspections

The available inspection types for the joints are:

- Cp/Cpk ISO

- SPC (joint)

It is possible to save two inspection with the same name and the same target objet.

A warning message is displayed to advise the operator an inspection with the same name already exists.

Select Yes to save the inspection.

Select No not to save the inspection.

In this Section

- Adding a Joint inspection
- Cp/Cpk ISO parameters
- SPC (joint) parameters
- Adding Joint check inspection(s) through the template file
- Deleting an inspection
- Editing a Joint inspection
- Running a Joint inspection

## Applies to: