# Adding Joint check inspection(s) through the template file

1. Generate the Template file for inspections and save it on a PC (for more information, see Generating Tool check / Joint check template).

2. On the PC, open the file STpad_JointnspectionImportFile.xlsm. The following is displayed:

3. Complete the file STpad_JointInspectionImportFile.xlsm to define the necessary inspection(s).

   When all the mandatory fields are filled in, the Wrong field column becomes green.

   The file STpad_JointInspectionImportFile.xlsm defines not only inspection(s), but also the linked joint(s). These are automatically imported on the device through the file STpad_JointInspectionImportFile.stpad.

   Check the Excel option for the workbook calculation. Open a Excel file and click File > Options. On left side of the Excel options dialog box, select Formulas > Automatic option for the Calculation options section.

4. When the Wrong field column in correspondence of the new inspection(s) is green colored, click the blue button Sort and export to automatically generate the file STpad_JointInspectionImportFile.stpad.

   The file STpad_JointlnspectionImportFile.stpad is automatically saved on the PC.

   Only the STpad_JointInspectionImportFile.stpad can be correctly imported on the device (for more information about how to import inspections, see Import inspections).

5. Save the file STpad_JointInspectionImportFile.xlsm.

6. Close the file STpad_JointInspectionImportFile.xlsm.

7. Import the inspection(s) saved in the file STpad_JointInspectionImportFile.stpad on the device (for more information about how to import routes, see Importing the inspection(s) on the device).

8. Click the Menu icon > Joints to check the import of the inspection(s) is correctly done.

## Applies to: