# Connecting the device to the IRC-Connect

1. Pair the IRC-Connect to be connected to the device (for more information, see the paragraph Pairing the IRC-Connect).

2. In the Toolbar, tap Measuring Devices.

3. In the Measuring devices page, tap the IRC-Connect to be connected to the device.

4. On the upper-right corner of the Edit IRC-Connect page, tap the More option icon (). Then tap Connect.

   If the connection process succeeded, on the upper-right corner of the device screen the IRC-C icon is shown.

   In the Measuring device page, the Connection of the IRC-Connect is Connection up.

   To open the Measuring device page, tap the left arrow near Edit IRC-Connect.

After each connection, in the General section of the Edit IRC-Connect page the firmware version of the IRC-Connect is updated.

## Applies to: