# Editing a Joint

1. From the Joints page, tap an existing joint.

   The following is displayed:

   A | Categories |  |

2. In the categories (General, Torque, Angle, Inspections) of the Edit joint page, edit the necessary parameter(s) according to customer needs.

3. On the upper-right corner of the Edit joint page, tap the Save icon ().

   The Save icon is available after one item has been edited.

Tap the More options icon > Linked inspection to displayed all the tool inspection linked to the joint.

## Applies to: