# Measuring devices

The measuring devices section describes how to connect the device to the related measuring device: STwrench and IRC-Connect.

The STwrench and IRC-Connect need the bluetooth connection to be used.

The device can store up to 100 measuring devices into its own memory.

Tap the Menu icon in the Toolbar. Then, select Measuring Devices from the Menu list.

The following is displayed:

A | Command button | B | List of measuring devices

In each row, the following information are shown:

- Name of the measuring device paired to the device.

- Serial number of the measuring device paired to the device.

- Type of the measuring device paired to the device. The available types are STwrench and IRC-Connect.

- Connection of the measuring device: The available status are: not paired, paired, connection up, connection down.

  The Connection is Not paired if the measuring device is configured but the pair has never been perform.

  The Connection is Paired if the pair has been perform but the connection has never been perform.

  The Connection is Connection up if the measuring device is connected to the STpalm.

  The Connection is Connection down if the measuring device connected to the STpalm is off or out of range.

For each measuring device type, only one Measuring device per time can be connected to the device.

In this Section

- Deleting a Measuring devices
- Searching a Measuring device
- IRC-Connect
- STwrench

## Applies to: