# Connecting the device to STwrench

1. Pair the STwrench to be connected to the device (for more information, see Pairing STwrench)

2. In the Home page, tap the More icon ().

3. In the Measuring devices page, tap the STwrench to be connected to the device.

4. On the upper-right corner of the Edit STwrench page, tap the More icon then Connect.

   If the connection process succeeds, on the upper-right corner of the device screen the STw icon is shown and on the STwrench display the IRCW icon is shown

To open the Measuring device page, tap the left arrow near Edit STwrench.

In the Measuring device page, the status of the STwrench is Connection up.

If the STwrench is added on the device memory, but it is not paired, in the Measuring Devices page, the Status of the STwrench is Not paired.

If the STwrench is paired to the device, but it is not connected, in the Measuring Devices page, the Status of the STwrench is Paired.

If the STwrench is connected to the device, but it is either off or out of range, in the Measuring Devices page, the Status of the STwrench is Connection down.

## Applies to: