# Adding a Tool inspection

1. In the Tools page, select a Tool already configure.

2. On the upper part of the Edit tool page, tap Inspections.

3. On the upper-right corner of the Inspections page, tap the Add icon ().

4. In the Test type window, select a inspection type.

5. In the General category of the Add Cm/Cmk inspection page, configure the general parameters of the inspection:

6. On the upper part of the Add inspection page, tap Torque

7. In the Torque category, configure the torque parameters of the inspection.

8. On the upper part of the Add inspection page, tap Angle .

   For the Pulse tool, this category is replaced by the Pulse category. Refer to step 12 of this procedure for the Pulse category configuration.

9. In the Angle category, configure the angle parameters of the inspection.

10. On the upper part of the Add inspection, tap More option icon (). Then, select Time.

11. In the Time category, configure the time parameters of the inspection.

12. In the upper part of the Add inspection, tap More option icon (). Then, select Pulse.

    This category is displayed only for the Pulse tools.

13. In the Pulse category, configure the pulse parameters of the inspection.

14. In the upper part of the Add inspection, tap the More options icon (). Then, select Picture.

15. In the Picture category, it is possible to:

    - Add an image/video: connect the STpalm to a PC. In the Download folder of the STpalm add a new folder named media_items and save in this folder the image/video to upload. In the Picture category of the Add inspection page, tap the Add icon () and select the media to upload.

      The maximum size of images is 5 MB, the maximum size of videos is 10 MB.

    - Remove an image/video: on the upper part of the Picture category, tap the Remove icon ().

16. In the upper part of the Add inspection, tap the More options icon (). Then, select Traceability.

17. In the Traceability category, configure the following parameters

    - Verification code: type the verification code that must be entered or scanned when the inspection is run. This field is case-sensitive.

    - Verification code description: to guide the operator, type the description of the verification code dialog box that is displayed when the inspection is run.

    Assignable causes: it is possible to:

    - List:

      - select an assignable causes list: tap the Search icon () and then select an already configured item in the Assignable causes list page.

      - add a new assignable causes list: tap the Search icon (); on the upper-right corner of the Assignable causes list page, tap Add to configure a new item.

      - delete the link to the assignable causes list: tap the Delete icon ().

    - Mandatory: if the check box is selected, the operator must select/type an assignable cause to continue the test.

    - Force selection from list: select between:

      - No: the operator can type the assignable cause, without selecting it from the list.

      - Yes: the operator can only select the assignable cause from the list.

      - Inherit: the selection from list can be forced or not forced, depending on the definition of this parameter in the Assignable causes list page.

    Corrective actions: it is possible to:

    - List:

      - select a corrective actions list: tap the Search icon () and then select an already configured item in the Corrective actions list page.

      - add a new corrective actions list: tap the Search icon (); on the upper-right corner of the Corrective actions list page, tap Add to configure a new item.

      - delete the link to the corrective actions list: tap the Delete icon ().

    - Mandatory: if the check box is selected, the operator must select/type a corrective action to continue the test.

    - Force selection from list: select between:

      - No: the operator can type the corrective action, without selecting it from the list.

      - Yes: the operator can only select the corrective action from the list.

      - Inherit: the selection from list can be forced or not forced, depending on the definition of this parameter in the Corrective actions list page.

18. On the upper-right corner of the Add inspection page, tap Save.

## Applies to: