# Importing joint check inspections on the device

1. Connect the STpalm to the PC via USB cable.

2. In the Autoplay dialog box, select Open the device to see the files> Internal shared storage > Download > .

3. In the Download folder of the STpalm, copy the STpad_ToolInspetionImportFile.stpad.

4. On the left side of the STpalm Toolbar, tap the Menu icon () > Configuration > Import / Export > Import Joint check inspections.

5. In the Import page, tap the Import file button.

6. On the File import message, tap OK.

   If the OK button is tapped, the database of the application is overwritten by the new tools and inspections. All the elements configured before the import are deleted.

7. On the Import results dialog box, tap OK.

   The import results dialog box lists the status of the import of each joint and inspection configured in the import file.

## Applies to: