# Quick programming

Quick Programming is a function that starts a test in a short time.

Before starting the quick programming test, connect the device to the related measuring device (for more information, see “Measuring devices”).

In case the device is connected to the IRC-Connect, do the “quick programming” test through one of the following transducers: IRTT, IRTT T/A.

The device automatically creates a default inspection (associated to a default tool) according to the tool, the connected transducer and the selected tool strategy.

For IRTT, IRTT T/A, the following tool strategies are available: Click wrench – Click wrench, Peak – Peak, Power tool – Direct driven, Pulse tool – Pulse tool, Pulse tool – ACTA Pulse tool, Click wrench - Cam-over, Power tool - Only angle.

It is possible to change the default inspection / tool that define the quick programming test, according to customer needs. Moreover, users can also save the default inspection / tool in the related sections.

In this Section

- Running a quick programming

## Applies to: