# Editing a Joint inspection

1. From the Inspections page, tap an existing inspection.

2. In the categories ( General, Torque, Angle, Time, Traceability) of the Edit inspection page, edit the necessary parameter(s) according to customer needs.

3. On the upper-right corner of the Edit joint page, tap the Save icon ().

   The Save icon is available after one item has been edited.

   If the inspection is sent by an external software, it is not possible to edit it.

## Applies to: