# EHMI Description

The EHMI (Extended Human Machine Interface) is located on the wrench controller and consists of a touch-sensitive control display and a push button. The display serves as a tool-integrated interface for the operator, and can be used to configure, select and run inspections and routes; to display tests' results and traces; and to configure device settings.

Position | Name | Definition
--- | --- | ---
1 | Display | Touchscreen serving as a tool-integrated interface for the operator.
2 | ON/OFF / Barcode | Physical button for turning on/off the wrench and for triggering the barcode scanner.

In this Section

- Indicator bar