# Reading the Trace Category

Position | Name | Definition
--- | --- | ---
1 | Upper limit | Upper limit value for the function under control.
2 | Result | Test result value. If the Double result function is enabled, both the residual point and the peak point are shown in the plot.
3 | Lower limit | Lower limit value for the function under control.
4 | Inspection name | Name of the selected inspection.
5 | Full-screen button | Button for opening a full-screen view of the plot. In full-screen mode, it is possible to select and zoom in on a section of the curve.
6 | Plot type button | Button for selecting the plot type to be displayed. Default plot is Torque over Angle.
7 | Next button | Button for moving to the trace of the next result inside the inspection.
8 | Previous button | Button for moving to the trace of the previous result inside the inspection.
9 | Test number | Number of the test inside the inspection.
10 | Batch count | Number of times the test has been run inside the inspection.