# Exporting and Importing Configurations

The export and import functions are used to export events and tightening results for analysis in external programs, as well as allowing for transferring of tightening programs, batches, and tool configurations between tools.

The export function is used to:

- Export tightening results and events for further processing.

- Export log files for debug assistance from an Atlas Copco service engineer.

- Export tool configuration that can be used to copy settings to another tool.

Export a configuration

1. Go to Integrated Controller Tool in the home menu. Select Export/Import in the left pane.

2. Select what to export from the tool: All information or Settings and configurations.

   When Settings and configurations is chosen no file with results or events will be exported into the archive. With this setting the export takes less time to perform.

3. Select EXPORT. A prompt to select where to save or retrieve the exported file is shown.

Import a configuration

1. Go to Integrated Controller Tool in the home menu. Select Export/Import in the left pane.

2. Select IMPORT. When using the import function, all settings for tightening program, batch, accessories, and tool are replaced by the settings from the import file. However, settings for network, PIN, and results and events are not imported.

3. Select CONTINUE in the dialog box to start the import.

In this Section

- Exported information and File Format