# A - Angle

This step monitor measures the maximum angle reached during the monitor and checks that it is between High limit and Low limit. The angle measurement starts at the start of the monitor or, if specified, at the point where the torque passes Trigger torque for the first time during the monitor.

Parameter | Description
--- | ---
Stop condition | Two stop condition types are available: Peak angle, Angle at peak torque (default).
Trigger torque | The angle measurement starts at this trigger.
Low Limit | Lowest acceptable angle.
High Limit | Highest acceptable angle.