# Torque

This strategy guides the operator in reaching the desired target torque, without any angle reading.

Parameter | Description
--- | ---
Required tag number | A specific number must be written in the TAG of the end fitting tool.
Name | Name of the tightening program.
Program start | Torque value from which the tightening operation starts. Must be ≥ smartHEAD Min torque value. If Program start = 0, its value is automatically set to the smartHEAD Min torque value.
Torque min | Lower torque limit.
Torque max | Higher torque limit.
Maximum torque limit | If the torque applied reaches this limit, the message Change screw is shown on the wrench display. Must be > Torque max.
Target torque | The torque target.
Torque units | This parameter is not editable.
Torque correction coefficient | When extensions are used, the wrench measurement might be compensated to show a more accurate torque value. To calculate the correction coefficient, please refer to How to calculate the Torque Correction Coefficient. The parameter is stored in the RFID TAG of the end fitting tool. When extensions are not used, Torque correction coefficient = 1.
Batch size | Number of tightenings the batch will perform. Maximum value: 99. If Batch size = 0, the number of tightenings is infinite. If Batch size > 1, batch result OK only if all tightenings are OK.
Max consecutive NOK | Number of accepted NOK to have an OK result.
End cycle time | Starts when the torque goes below the Program start after reaching the 3rd percentage. Default value: 0.1 sec. Minimum value: 0.1 sec. Maximum value: 5 sec.
Ratchet time | Starts when the torque goes below the Program start without reaching the 3rd percentage value. This allows the operator to release the torque for a while and recharge during the tightening operation. Default value: 5 sec. Minimum value: 0.1 sec. Maximum value: 30 sec.

Torque vs. Time

A | Torque max | B | Target torque
C | Torque min | D | Program start

The green area indicates the OK result area.
The torque result is the maximum torque measured during the tightening.

During the tightening operation, LEDs, buzzer and vibration are activated as follows:

- LEDs:

  - First radial gradient LEDs white (two directions): torque over 1st percentage (30% of the Torque min).

  - Second radial gradient LEDs white (two directions): torque over the 2nd percentage (60% of the Torque min).

  - Third radial gradient LEDs white (two directions): torque over the 3rd percentage (95% of the Torque min).

  - All three radial gradient LEDs green: torque between Torque min and Torque max.

  - All three radial gradient LEDs red: torque over Torque max.

  Torque vs. Angle

  A | Torque max | B | 3rd percentage
  C | 2nd percentage | D | 1st percentage

- Buzzer

  - The beep starts when the torque goes over the Program start value; the signal increases when the 1st percentage, the 2nd percentage, the 3rd percentage, and the Torque max are reached.

- Vibration:

  - Starts together with the third radial gradient LEDs.

At the end of the tightening operation, LEDs, buzzer and vibration are activated as follows:

- LEDs:

  - Blue LEDs: torque result between Program start and Torque min.

  - Green LEDs: torque result between Torque min and Torque max.

  - Red LEDs: torque result over Torque max.

- Buzzer

  - Two beeps indicate the end of the operation; if the final result is in the red area, the signal in continuous.
    To stop the buzzer, start a new tightening operation or press a button on the tool controller.

- Vibration:

  - Stays active until the torque applied is released.

Relevant Information

- How to Calculate the Angle Correction