# Configuring a Wireless Client

1. Go to Settings in the home menu and select Network in the left pane.

2. In the Wireless Client field, select Edit.

3. Set Enabled to On.

4. Set DHCP to On or Off depending on the configuration. If set to Off, fill out the required information, provided by the local system administrator:

   - IP address

   - Subnet mask

   - Gateway

5. Enter a Network name (SSID).

6. In the Security field, select Mode and choose a security mode from the list. If WPA2 Personal is chosen, enter a Security key.

7. Enter security parameters and import cert files and keys, as applicable.

8. Edit the Optional Settings as applicable.

9. Select Apply.

   The tool will establish a wireless connection to the network, indicated with the tool's blue connection LED indicator emitting a steady light.

10. To access the user interface wirelessly, type the IP address into a web browser.

## Product Essentials Tutorials

https://www.youtube.com/watch?v=IAhVDKSyFgY