# Getting Started

To create a better overview of the system, this section provides a quick guide covering the basic steps required to get started with the STRwrench and STRwrench Web Interface . The section does not explain every feature of the system, but instead focuses on the most basic ones.

Get started

1. Connect the tool to a PC and access the web user interface. Set up a wireless connection between the tool and the Power Focus.

2. On the Power Focus, define a tightening program containing all relevant parameters of a tightening, for example target angle and target torque.

   If applicable, create a batch sequence. One or several tightening programs can be added to a batch sequence which works as a series of tightening programs. A batch sequence can for example be a certain number of tightenings with a tightening program, or a sequence of different tightening programs.

3. Assign a tool and a task to the virtual station. The task can be either a tightening program, a batch sequence, or a specified digital input (from for example a barcode scanner).

In this Section

- Accessing the STRwrench Web Interface
- Creating a Tightening Program
- Assigning a Task to the Virtual Station