# General Settings

Item | Description
--- | ---
Front LED | On: Front LED is lit when the dedicated button is pressed. Off: Front LED will always be off.
TAG selection | On: Select the Tightening Program/Batch or Batch Sequence according to the TAG number configured in the Batch Sequence/Source Tightening/Source Batch. Off: The tool does not select the Tightening Program/Batch or Batch Sequence.
TAG | On: Information on the TAG is displayed and can be edited in the Integrated Controller Tool > Tool menu. Off: Information on the TAG will not be displayed.
Buzzer | On: Audio signaling device will always be on. Off: Audio signaling device will always be off.
Vibration | On: Vibrating device will always be on. Off: Vibrating device will always be off.
Loose pre-tightening check | On: Accidental unscrewing of an already tightened joint is detected before the tightening starts. Off: Function deactivated.