# Installation Overview

Legend to page 2.

To install the insulated tool cover, do the following:

1. Remove the front nut and the rubber ring from the insulated tool cover.

2. Separate the insulated tool cover in its two halves.

3. Attach the two halves of the insulated tool cover to the tool.

4. Fasten the front nut and attach the rubber ring in place onto the tool.

To remove the insulated tool cover, do the following:

1. Remove the front nut and the rubber ring of the insulated tool cover from the tool.

2. Remove the two halves of the insulated tool cover from the tool.