# Event Codes

Different types of events are used to notify the user of certain state changes or occurrences in the system. Each event requires a different action.

Some of the procedures described can only be performed by Atlas Copco Service personnel.

For more information about a specific event code, use the below filters or enter the event code search criteria in the search box.

Event Code
Event Type
Event Name
Description
Procedure
Log / Display / Ack / Conf
Available for
Group
Search

Event Code | Event Type | Event Name | Description | Procedure | Log / Display / Ack / Conf | Available for | Group
--- | --- | --- | --- | --- | --- | --- | ---
none | item | none | none | none | column | list | list
1000 | Info | Controller Started | The controller is started. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Controller and Tool
1001 | Warning | Controller Serial Number Updated | Generated at start-up if IT-board box serial number (controller serial number) differs from AUX-board box serial number. AUX-board is considered to be non-replaceable in field. The controller will reboot when the serial number is updated. | Replace IT-board or box. | Log Display Ack Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller and Tool
1010 | Info | Tool Connected | A tool is connected. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Controller and Tool
1011 | Info | Tool Disconnected | A tool is disconnected. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Controller and Tool
1012 | Info | Tool Rejected Controller Connection | This event can occur if the tool is into a skip-zone. | Verify if another controller is connected to the tool. Make sure that the tool settings are correctly set up. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller and Tool
2000 | Warning | Battery Low |  | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2001 | Warning | Battery Empty |  | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2002 | Warning | Tool Battery Health Low | Tool battery health problem is detected. Valid for SRB, TBP and IxB tools only. | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2004 | Warning | Tool is not of the preferred type | Tool has been replaced by a tool with a different Tool Max Torque. | Change tool. | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2006 | Warning | Tool Backup Battery Health low | The backup battery in the tool has too poor performance. | The backup battery should be replaced. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2007 | Warning | Tool Backup Battery Missing | Tool backup battery is missing. Valid for SRB, TBP and IxB tools only. | Insert battery | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2008 | Warning | Tool Backup Battery Error | Tool backup battery error detected. Valid for SRB, TBP and IxB tools only. | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2009 | Warning | Backup Battery Voltage Low | The controller's backup battery is almost empty | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2010 | Error | Tool Software Version Mismatch | Tool and controller software versions not compatible. | Service tool - update tool software. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2012 | Warning | Tool Communication Disturbance | Communication between tool and controller interrupted. | Relocate antenna placement. | Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Tool
2013 | Warning | Illegal Ring Position | Tool direction switch in faulty position. | If occurring frequently - service the tool. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2014 | Warning | Tool Overheated | Tool overheated. Valid for SRB, TBP and IxB tools only. | Allow tool to cool down. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2015 | Error | Tool Temperature Sensor Error | SRB, TBP and IxB tools only. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2016 | Warning | Tool Pulse Unit Overheated | Pulse unit overheated. Tool is not locked, but the warning is displayed whenever the tool is started as long as the pulse unit temperature is over threshold. Valid for SRB, TBP and IxB tools only. | Allow tool to cool down. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2019 | Warning | Tool Could not Start Motor | Tool motor failure. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2020 | Warning | Tool Requires Motor Tuning | Tool requires motor tuning. | Perform a motor tuning. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2021 | Warning | Motor Tuning Failed | Motor tuning failed. | Complete motor tuning or service the tool. | Log | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2022 | Info | Motor Tuning Completed | Motor tuning completed. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2023 | Warning | The Tool Requires Open End Tuning | The tool requires open end tuning. | Perform open end tuning. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2024 | Warning | Open End Tuning Failed | Open end tuning failed. | Try to perform open end tuning one more time. If it fails again, service the tool. | Log Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2025 | Info | Open End Tuning Successful | Open end tuning successful. |  | Log Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2026 | Warning | Open End Position Failed | Open end position failed. | Press the tool trigger again and wait for the positioning to be completed. If it fails again, service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2027 | Warning | Usage Limited Due To High Tool Temperature | Temperature limit value has been reached. Tightening has been inhibited to reduce risk for tool shutting down due to overheating. | Wait until tool temperature has been reduced. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2030 | Error | Tool Memory Failure: Change Tool | Tool memory corrupt. | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2031 | Error | Tool Accessory Memory Corrupt | Tool accessory memory corrupt. | Service the tool accessory. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2040 | Error | System Check Failure |  |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2041 | Error | Torque Transducer Error | Will be generated either on calibration error or if tool reports transducer error. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2042 | Error | Angle Transducer Error |  | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2043 | Error | Tool Ground Fault Error |  | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2044 | Info | Tool Service Interval Expired | Indicates that servicing of the tool is needed. Triggered when the number of set tightenings has been exceeded. | Perform service of tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2045 | Warning | Tool Calibration Data Invalid | If validation of calibration data fails. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2046 | Info | Tool: Next Calibration Date Has Passed | Indicates that calibration of tool is needed. Triggered when calibration alarm is enabled in settings and the current time is greater than next calibration date. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2048 | Info | Tool Calibration Value Updated By QA Device | Tool calibration was updated when a calibration with a QA device was performed. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2050 | Error | Tool Parameter File Not Supported | Required tool parameters are missing. | Update tool parameters. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2060 | Info | Unexpected Trigger Behavior | Used to prevent start of tool if accessory is connected. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2071 | Error | Tool Memory Corrupt | Tool descriptor is corrupt. | Service the tool. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2072 | Info | Unknown Device Connected |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2073 | Warning | Tool Trigger Supervision Failure | HW channel failure. Mismatch between hardware and software of tool trigger. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2074 | Warning | Tool Indicator Board Failure | Tool indicator board failure. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2075 | Warning | Tool Fan Voltage Failure | Tool fan voltage failure. | Service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2076 | Warning | Tool Accessory Bus Voltage Failure | Tool accessory bus voltage failure. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2077 | Warning | Tool Trigger Sensor Error | Tool trigger sensor error. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2078 | Info | Tool Tightening Program Updated | Tool locked due to tightening program update. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2079 | Error | Tool Cable Not Supported | Tool cable is corrupt. The chip in the cable is not responding or is damaged. | Switch cable. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tool
2080 | Error | Tool Battery Failure | DC voltage too high or too low. Battery failure. | Contact the Atlas Copco service representative and send back battery to Atlas Copco (do not reuse it!). | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2081 | Error | Tool Current Limit Reached | The current limit value has been reached and the drive is disabled. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2082 | Error | Tool Current Measurement Error | Current measurement error. Current cannot be measured with a reliable result. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2083 | Error | Tool Internal Error | Various internal hardware errors. Valid for STB and IxB tools only. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2084 | Error | Tool Internal Software Error | Various internal software errors. Valid for STB and IxB tools only. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2085 | Error | Tool RBU Error | An RBU error was detected by the tool software. | Check that the RBU is correctly installed. If error is still present then service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2086 | Error | Tool Stall | Tool motor is stalling. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2087 | Warning | Tool Motor Current High | Tool motor current limit value is exceeded, and the tool is locked. Tool will enter failsafe mode. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2088 | Warning | Tool Battery Current High | Tool battery current is too high. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2089 | Warning | Tool Drive Voltage Low | Tool drive voltage is below the monitored lower voltage limit value. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2090 | Warning | Tool Drive Voltage High | Tool drive voltage is above monitored higher voltage limit value. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2091 | Warning | Tool Main Board Error | Tool main board internal error. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2092 | Warning | Tool Power Module Error | Tool power module internal error. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2093 | Warning | Pulse Unit Oil Level Low | The oil level of the connected pulse tool is low. | Service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2094 | Warning | Pulse Unit Oil Level Empty | The oil level of the connected pulse tool is below required operational level. | Service the tool. | Log Display Ack Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2095 | Warning | Tool Battery Communication Lost | Tool lost communication with battery. Valid for SRB, TBP and IxB tools only. | Make sure battery is snugged correctly. Otherwise change battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2096 | Error | Tool Battery Software Version Mismatch | Tool battery software incompatible with tool software. Valid for SRB, TBP and IxB tools only. | Update software. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2100 | Info | STwrench smartHEAD Removed | STwrench smartHEAD has been removed. | Reconnect smartHEAD and restart the wrench. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tool
2101 | Warning | Wrench Tightening When Locked | A wrench tightening was performed when the tool status was locked in the controller. | Wait until the tool status in controller is unlocked. | Log Display Conf | Power Focus 6000 Power Focus 8 | Tool
2120 | Warning | Unable To Start: Tool Has No Active Torque Transducer |  |  | Log Display | Flex | Tool
2121 | Warning | Transducers Are Disabled For Connected Tool |  |  | Log Display | Flex | Tool
2122 | Warning | Unable To Start: Tool Is Missing Required Torque Transducer |  |  | Log Display | Flex IxB | Tool
2123 | Warning | Unable To Start: Tool Is Missing Required Angle Transducer |  |  | Log Display | Flex | Tool
2124 | Error | Torque Transducer Error On Main Transducer | Shows that there is an error on the Main torque transducer of a Tool with dual transducers. |  | Log Display | Flex | Tool
2125 | Error | Torque Transducer Error On Secondary Transducer | Shows that there is an error on the Secondary torque transducer of a Tool with dual transducers. |  | Log Display | Flex | Tool
2126 | Error | Tool Torque Transducer Calibration Error On Main Transducer |  |  | Log Display | Flex | Tool
2127 | Error | Tool Torque Transducer Calibration Error |  |  | Log Display | Flex StepSync | Tool
2128 | Error | Tool Torque Transducer: Shunt Test Failed On Main Transducer |  |  | Log Display | Flex | Tool
2129 | Error | Tool Torque Transducer: Shunt Test Failed |  |  | Log Display | Flex StepSync | Tool
2130 | Error | Tool Torque Transducer: Zero Offset Compensation Failed On Main Transducer |  |  | Log Display | Flex | Tool
2131 | Error | Tool Torque Transducer: Zero Offset Compensation Failed |  |  | Log Display | Flex StepSync | Tool
2132 | Error | Tool Torque Transducer Hardware Error On Main Transducer |  |  | Log Display | Flex | Tool
2133 | Error | Tool Torque Transducer Hardware Error |  |  | Log Display | Flex StepSync | Tool
2134 | Error | Tool Torque Transducer Error: Overflow In A/D Converter On Main Transducer |  |  | Log Display | Flex | Tool
2135 | Error | Tool Torque Transducer Error: Overflow In A/D Converter |  |  | Log Display | Flex StepSync | Tool
2136 | Error | Tool Torque Transducer Calibration Error On Secondary Transducer |  |  | Log Display | Flex | Tool
2137 | Error | Tool Torque Transducer Error: Shunt Test Failed On Secondary Transducer |  |  | Log Display | Flex | Tool
2138 | Error | Tool Torque Transducer Error: Zero Offset Compensation Failed On Secondary Transducer |  |  | Log Display | Flex | Tool
2139 | Error | Tool Torque Transducer Hardware Error On Secondary Transducer |  |  | Log Display | Flex | Tool
2140 | Error | Tool Torque Transducer Error: Overflow In A/D Converter On Secondary Transducer |  |  | Log Display | Flex | Tool
2202 | Error | Tool HMI overcurrent occurred | Tool HMI overcurrent was detected. | Service the tool. Replace tool HMI. | Log Display Ack Conf | IxB | Tool
2203 | Error | Tool front light overcurrent occurred | Tool front light overcurrent was detected | Service the tool. Replace tool front light. | Log Display Ack Conf | IxB | Tool
2204 | Error | Accessory bus overcurrent occurred | Accessory bus overcurrent was detected. | Service the tool. Replace accessory bus. | Log Display Ack Conf | IxB | Tool
2207 | Error | Vibrator overcurrent occurred | Vibrator overcurrent was detected. | Service the tool. Replace the vibrator. | Log Display Ack Conf | IxB | Tool
2208 | Warning | System CPU temperature high | System CPU temperature high. | Wait until tool temperature has been reduced. | Log Display Conf | IxB | Tool
2209 | Error | System CPU temperature critical | System CPU temperature critical. | Wait until tool temperature has been reduced. | Log Display Conf | IxB | Tool
2210 | Error | Unsupported power source: tightening not permitted | Battery with too low voltage attached to the tool. | Attach battery with higher voltage to the tool. | Log Display Ack Conf | IxB | Tool
2217 | Info | Running on backup battery | Running on backup battery. |  | Log | IxB | Tool
2218 | Info | Battery connected | Battery connected or controller/tool started. |  | Log | IxB | Tool
2219 | Info | Power source: unknown | Unknown power source connected or controller/tool started with unknown power source. |  | Log | IxB | Tool
2500 | Error | Tensioner puller bar max number | Tensioner puller bar must be replaced. System is locked for usage. Pressure can only be released. | Send the tensioner to service organization for replacement of the puller bar. | Log Display Ack | PFHC | Tool
2501 | Error | Pump motor protection alarm | The pump motor protection has stopped the motor. The system must stop. If the system is under pressure, it needs manual actions to release pressure. | Turn off the system. If under pressure, mechanically release the pressure and send the pump to service. | Log Display Ack | PFHC | Tool
2502 | Error | Pump motor oil level low alarm | The pump motor oil level is low which has stopped the motor. If the system is under pressure, it needs manual actions to release pressure. | Turn off the system. If under pressure, mechanically release the pressure and top up oil. | Log Display Ack | PFHC | Tool
2503 | Error | Pump motor oil temperature high alarm | The pump motor oil temperature is high. | Turn off the system and wait for the oil to cool down. | Log Display Ack | PFHC | Tool
2504 | Error | Tensioner pressure sensor alarm | Failure in the pressure sensor electronics of the tensioner. No pressure can be read nor reported to the system. | Turn off the system. If under pressure, mechanically release the pressure and send the tensioner to service. | Log Display Ack | PFHC | Tool
2505 | Error | Pump pressure sensor alarm | Failure in the pressure sensor electronics of the pump. No pressure can be read nor reported to the system. | Turn off the system. If under pressure, mechanically release the pressure and send the pump to service. | Log Display Ack | PFHC | Tool
2506 | Error | Unexpected clockwise rotation detected | A clockwise nut rotation while waiting for pressure release after completed tensioning. The result is invalidated. | Release pressure and tension the nut again. | Log Display Conf | PFHC | Tool
2507 | Error | Unexpected counter clockwise rotation detected | A counter clockwise nut rotation while waiting for pressure release after completed tensioning. The result is invalidated. | Release pressure and tension the nut again. | Log Display Conf | PFHC | Tool
2508 | Error | Pump or tensioner pressure sensor failure | Too large difference between the pressure sensor readings in the pump and the tensioner. Pressurization is halted. | Problem in the hydraulics or the calibration of the pressure sensors. Restart the system and try again. If the problem repeats, contact your local Atlas Copco sales representative. | Log Display Ack | PFHC | Tool
2509 | Error | Tensioner pressure sensor failure or hydraulic hose failure | The tensioner's pressure sensor indicates no pressure but the pump's sensor reads a pressure increase. Pressurization is halted. | Problem in the hydraulics or the calibration of the pressure sensors. Restart the system and try again. If the problem repeats, contact your local Atlas Copco sales representative. | Log Display Ack | PFHC | Tool
2510 | Error | Set custom ID failed | Setting custom ID failed. | Restart the system and check the connected devices. If Custom ID for the unit is wrong, redo the setting. | Log Display Ack | PFHC | Tool
2511 | Info | Custom ID is set | Setting custom ID succeeded. |  | Log Display Ack | PFHC | Tool
2512 | Warning | Malformed Barcode string, ignored | The scanned string could not be parsed as a tower data bar code. | Scan a proper tower data qr code or scan tower section id. | Log Display Ack | PFHC | Tool
2513 | Error | No pump pressure detected | The system is trying to pressurize but no pressure increase is registered in the pump. Possible cause is incorrect phase order in the three phase connector. | Power off the system and reverse the phases of the power connector. | Log Display Ack | PFHC | Tool
2514 | Warning | Tensioner overtorque alarm | Too high torque is applied to the click wrench. This causes damage to the torque sensor. | Relax the torque. | Log | PFHC | Tool
2515 | Warning | Tensioner overpressure alarm | The pressure in the tensioner is too high. | Let the pressure drop, or release the pressure. Check the hydraulic pressure parameters. | Log | PFHC | Tool
2516 | Warning | Unexpected Pump or Tensioner firmware | Unexpected Pump or Tensioner firmware version detected, restart system. If the problem persists, the system may be possible to run, but carefully observe any unexpected behaviour. | Power cycle system | Log Display Ack | PFHC | Tool
2517 | Error | Incompatible Pump or Tensioner firmware version, restart system. The system cannot run. | Incompatible Pump or Tensioner firmware version, restart system. The system cannot run. | Restart system, if this doesn’t help replace the failing unit. Check connected devices to see which one has not connected. | Log Display Ack | PFHC | Tool
3000 | Error | Controller Internal Software Error | Software error in the controller. | Contact service. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3001 | Error | Controller Clock Battery Empty | Internal battery is getting close to end of life. | Replace battery. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3010 | Warning | System Overheated | The controller is overheated. | Cool down. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3011 | Warning | Drive Overheated Controller Hardware |  | Cool down. | Log Display Conf | Flex | Controller, Drive and StepSync
3013 | Warning | Usage Limited Due To High Controller Temperature | Temperature limit value has been reached. Tightening has been inhibited to reduce risk for controller shutting down due to overheating. | Wait until controller temperature has been reduced. | Log Display Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3020 | Warning | Controller Hardware Failure |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3021 | Warning | System Voltage Problem | DC voltage too high or too low. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3022 | Warning | Controller Voltage Problem: AC Input Voltage Too High | DC voltage too high or too low. | Fix the input voltage. | Log Display | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3023 | Warning | Controller Voltage Problem: AC Input Voltage Too Low | DC voltage too high or too low. | Fix the input voltage. | Log Display | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3024 | Warning | Drive Voltage Problem: AC Input Voltage Too High | DC voltage too high or too low. | Fix the input voltage. | Log Display | Flex | Controller, Drive and StepSync
3025 | Warning | Drive Voltage Problem: AC Input Voltage Too Low | DC voltage too high or too low. | Fix the input voltage. | Log Display | Flex | Controller, Drive and StepSync
3030 | Error | IP Address Conflicting With Another Node On The Network | The set IP address is in use by another device on the same network. | Change IP address on one of the devices. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Controller, Drive and StepSync
3031 | Info | Network Cable Unplugged | The carrier of the factory port is lost (cable disconnected). | Check the cable connection. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3032 | Info | Pairing Started | Tool pairing started. |  | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3033 | Info | Pairing Successful | Tool pairing successful. |  | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3034 | Info | Pairing Unsuccessful: No Tool Found | The controller found no tool to pair with when scanning for radio peers. | Set the tool in pairing mode and try again. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3035 | Error | Pairing Unsuccessful: More Than One Tool Found | The controller found more than one tool when scanning for radio peers. | Ensure that only one tool is in pairing mode when starting the pairing mode on the controller. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3036 | Error | Pairing Unsuccessful: Communication Error | The controller experienced a loss of connection, an unexpected answer or timeout during the pairing process. | Try to perform pairing one more time. If it fails again, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3037 | Info | Pairing Unsuccessful: Tool Slot Is Full |  | Clear one tool slot. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3040 | Warning | Emergency Stop | Drive disabled due to emergency stop. | Reset emergency stop. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3050 | Info | System Clock Updated | System clock has been updated. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Controller, Drive and StepSync
3051 | Error | System Clock Error | Wrong time read from hardware Real Time Clock (RTC). | Change RTC battery. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Controller, Drive and StepSync
3052 | Warning | Remote Start Configuration Error | Mismatch between HW and SW remote start configuration. | Verify that HW dip switch matches the selected start source. | Log Display Conf | Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3053 | Info | Drive Connected | StepSync drive has been connected. |  | Log Display | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3054 | Info | Drive Disconnected | StepSync drive disconnected. |  | Log Display | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3055 | Warning | Mode Configuration Error | Generated when selected mode is configured wrongly. E.g. configuring two bolts with the same bolt number or the same channel, incomplete mode configuration. | Check ToolsTalk 2 for mode configuration error. | Log Display | Flex StepSync | Controller, Drive and StepSync
3056 | Warning | Unable to Start: Tool Or Drive Is Missing | Generated when a used channel is missing a drive or tool. | Verify Channel Menu on the HMI. Connect missing drive or tool. | Log Display | Flex StepSync | Controller, Drive and StepSync
3057 | Info | Unable to Start: Channel Is Already In Use | Generated when a needed channel has been allocated to another virtual station. |  | Log Display | Flex | Controller, Drive and StepSync
3058 | Info | No Mode Selected |  | Select mode. | Log Display | Flex StepSync | Controller, Drive and StepSync
3059 | Warning | Failed To Connect To Atlas Copco License Manager | Indicates that the controller failed to connect to the local license manager to get licenses. | Verify the local network. If it fails again, service the controller. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3061 | Warning | Unable To Start: Enable Signal Is Low |  |  | Log Display | Flex StepSync | Controller, Drive and StepSync
3062 | Warning | Unable To Start: Stop Signal Is High |  |  | Log Display | Flex StepSync | Controller, Drive and StepSync
3063 | Warning | Unable To Start: All Channels Inhibited | All channels have been set inhibited, so no tightening can be started. | Set at least one channel to not be inhibited. | Log Display | Flex StepSync | Controller, Drive and StepSync
3064 | Warning | Carrier Number Faulty | A FlexCarrier hex switch is set to zero. | Turn the switch to a non-zero value. | Log Display | Flex | Controller, Drive and StepSync
3065 | Warning | Carrier E-Stop Configuration Plug Wrong Type Or Missing | A Carrier is missing its E-stop configuration plug, or the plug type is wrong. | Insert correct plug type. | Log Display | Flex | Controller, Drive and StepSync
3066 | Warning | Carrier Voltage Inlet: No 3-Phase AC |  |  | Log Display | Flex | Controller, Drive and StepSync
3067 | Warning | Carrier Voltage Inlet: One AC Phase Missing |  |  | Log Display | Flex | Controller, Drive and StepSync
3068 | Warning | Carrier: Internal 24 VDC Power Supply Unit Broken |  |  | Log Display | Flex | Controller, Drive and StepSync
3069 | Warning | Carrier 24 Voltage OUT-Port Disabled Due To Over-Current |  | Reset the system. | Log Display | Flex | Controller, Drive and StepSync
3070 | Warning | Carrier, Hardware Error In PF6 FlexControl Cable OUT |  | Reset the system. | Log Display | Flex | Controller, Drive and StepSync
3071 | Warning | Carrier, Hardware Error In PF6 FlexControl Cable IN |  | Reset the system. | Log Display | Flex | Controller, Drive and StepSync
3072 | Warning | Emergency Stop 24 VDC Power Failure Due To Short-Circuit |  |  | Log Display | Flex | Controller, Drive and StepSync
3073 | Warning | Unable To Start: System Is Emergency Stopped | When allocating multiple spindles, this event is invoked by "preStartCheckFailed" due to emergency stop. | Reset the emergency stop. | Log Display | Flex StepSync | Controller, Drive and StepSync
3074 | Warning | Carrier Overheated |  |  | Log Display | Flex | Controller, Drive and StepSync
3075 | Warning | Carrier Temperature OK |  |  | Log Display | Flex | Controller, Drive and StepSync
3076 | Warning | Carrier: Internal 24 VDC Power Supply Overload | Current output from internal PSU is too high. | Disconnect other carriers that are powered from the PSU. Disconnect any external equipment using 24 VDC. | Log Display | Flex | Controller, Drive and StepSync
3077 | Warning | Carrier: Internal 24 VDC Power Supply Over Voltage | Voltage output from internal PSU is too high. | Replace the carrier. | Log Display | Flex | Controller, Drive and StepSync
3078 | Warning | Carrier: Internal 24 VDC Power Supply Under Voltage | Voltage output from internal PSU is too low. | Replace the carrier. | Log Display | Flex | Controller, Drive and StepSync
3079 | Warning | External Supply To Carrier: 24 VDC Over Voltage | Backup input voltage is more than 27 VDC. | Adjust the backup input voltage. | Log Display | Flex | Controller, Drive and StepSync
3080 | Warning | External Supply To Carrier: 24 VDC Under Voltage | Backup input voltage is less than 19 VDC. | Adjust the backup input voltage. | Log Display | Flex | Controller, Drive and StepSync
3081 | Warning | Carrier Voltage Inlet: 3-Phase AC Over Voltage | Input voltage is too high. | Lower input voltage: must be 400 VAC or 480 VAC. | Log Display | Flex | Controller, Drive and StepSync
3082 | Warning | Carrier Voltage Inlet: 3-Phase AC Under Voltage | Input voltage is too low. | Higher input voltage: must be 400 VAC or 480 VAC. | Log Display | Flex | Controller, Drive and StepSync
3083 | Error | Wrong Anybus/Profisafe Module Firmware |  |  | Log Display | Flex Power Focus 6000 Power Focus 8 StepSync | Controller, Drive and StepSync
3084 | Error | Soft PLC Runtime Error | eCLR has terminated in an uncontrolled way. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Controller, Drive and StepSync
3085 | Warning | Carrier: Fan Module Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3086 | Warning | Carrier: Fan Module Partly Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3087 | Warning | Carrier: Left Fan Module Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3088 | Warning | Carrier: Left Fan Module Partly Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3089 | Warning | Carrier: Right Fan Module Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3090 | Warning | Carrier: Right Fan Module Partly Out Of Order |  |  | Log Display | Flex | Controller, Drive and StepSync
3096 | Warning | Cellular signal strength low | The RSSI value for the cellular connection is under the defined threshold value of -98 dBm. | Move the tool closer to the cellular antennas for a stronger connection and avoid data loss. | Conf | IxB | Controller, Drive and StepSync
3097 | Warning | Cellular connection lost | The system lost connection to the cellular network. | Move the tool closer to the cellular antennas. Check the cellular connection setup so correct APN is still configured. Check the cellular network for any problems. | Log Display Conf | IxB | Controller, Drive and StepSync
3100 | Warning | Mode Configuration Does Not Exist |  |  | Log Display | Flex StepSync | Controller, Drive and StepSync
3150 | Error | Software IAM Incompatibility | IAM is incompatible with the software that is installed on the controller. | Replace IAM. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3160 | Error | Failed To Activate Newly Installed Software | Something went wrong during the activation. When the newly installed software starts, a fallback to the previous working software happens. This error happens when the new software fails to start for three times and only during software installation. | Take an export and contact Atlas Copco for further assistance. Note down the software version you are trying to install as well as the software version that is working. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3161 | Error | Started On Unexpected Software Partition | The controller has started on the inactive software side and not on the expected software side. | Note down the software information (on the Home screen of the controller, select Controller > Software). Try to restart the controller and make sure its running on correct software when started again. If error persists, do an export and contact Atlas Copco. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3500 | Error | Generic License Manager Error | Inconsistency detected in the feature management system used. | Contact Atlas Copco representative. | Log Display Ack | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3501 | Error | License Manager Synchronization Error |  |  | Log Display Ack | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3502 | Info | License Manager Synchronization Done |  |  |  | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3503 | Warning | License Manager: Another Source in Use | License is used by another source. | Verify license assignment. | Log Display | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3504 | Warning | License Manager Restart Needed |  | Restart license manager. | Log Display | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3505 | Info | USB License Synchronization Started |  |  | Log | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3506 | Error | USB License Synchronization Error |  |  | Log | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and StepSync
3507 | Info | USB License Synchronization Done |  |  | Log | Power Focus 6000 Power Focus 8 | Controller, Drive and StepSync
3508 | Info | One or more of your licenses are about to expire. Please make sure you have a license server configured |  | Update licenses. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3511 | Warning | One of your licenses has a different license definition | Inconsistency detected in a license to be used. | Contact Atlas Copco representative. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3550 | Warning | License Is Missing |  | Install the correct license. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
3551 | Warning | Wireless Communication Disabled By Licensing |  | Unassign Standalone license from the Virtual Station. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Controller, Drive and StepSync
4010 | Info | Tool Locked By Digital Input | The tool is locked by a digital input signal. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4011 | Info | Tool Locked By Open Protocol | The tool is locked by Open Protocol. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4012 | Info | Tool Locked By Fieldbus | The tool is locked by the Fieldbus. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4013 | Info | Tool Locked By Socket Selector | Tool is locked when the socket selector is disconnected from the Virtual Station. | Unlock by Master Unlock. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4014 | Info | Tool Locked By Soft PLC | Soft PLC signal locked the tool. | Unlock by Master Unlock. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4015 | Info | Loosening Disabled | Loosening is disabled in the tightening program. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4016 | Info | Tightening Disabled |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4017 | Info | Loosening Not Configured | Loosening is not configured in the selected tightening program | Select different tightening program. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4020 | Info | Too Many NOK Tightenings | Maximum consecutive NOK tightenings in batch is exceeded |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4025 | Info | No Tightening Program Selected | No tightening program selected. | Select tightening program or batch sequence. | Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4030 | Info | Batch Sequence Aborted | The batch sequence has been aborted. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Tightening Process
4031 | Info | Max Time To Complete Batch Sequence Reached |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4032 | Info | Max Time To Complete First Tightening Reached |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4035 | Info | Locked By Line Control |  |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4040 | Info | Locked By Alternative Identifier | Tool locked by alternative identifier. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4050 |  | Invalid Socket Configuration | Tightening program assigned to multiple sockets. | Tightening program assigned to multiple sockets. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4060 | Info | Tool Locked On Batch Complete | When running a batch with flag Tool lock on batch sequence complete this event is generated when the user press the trigger. | Unlock with signal Unlock Tool on complete. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4070 | Info | Process Enter Manual Mode | Indicates that manual mode has been activated for a virtual station. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4071 | Info | Process Enter Automatic Mode | Indicates that automatic mode has been entered for a virtual station. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4072 | Info | Test Bolt |  |  | Conf | Flex StepSync | Tightening Process
4073 | Info | Tool zero position updated | Indicates that the tool zero position is set using signals. |  | Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4100 | Warning | Identifier Not Accepted: Invalid String Length |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4101 | Warning | String Selection Unsuccessful: Multiple Matches |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4102 | Warning | String Selection Unsuccessful: No Match Found |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4103 | Warning | Identifier Not Accepted: Identical String Already Received |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4104 | Warning | Identifier Not Accepted: No Match Found |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Tightening Process
4500 | Info | Result DriveError | Internal driver error or driver loss detected. |  | Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4501 | Info | Result Rehit | Attempt to tighten an already tightened bolt when Rehit detection is on. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4502 | Info | Result Soft Start Torque Low | Soft start torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4503 | Info | Result Soft Start Torque High | Soft start torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4504 | Info | Result Self Tap Torque High | Self-tap torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4505 | Info | Result Self Tap Torque Low | Self-tap torque below minimum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4506 | Info | Result Safety Torque Low | Automatically calculated torque value to ensure torque sensor is mounted correctly. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4507 | Info | Result Rundown Torque High | Rundown torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4508 | Info | Result Rundown Angle High | Rundown angle exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4509 | Info | Result Rundown Time High | Rundown time exceeded maximum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4510 | Info | Result Rundown Time Low | Rundown time below minimum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4511 | Info | Result Rundown Torque Low | Rundown torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4512 | Info | Result Rundown Angle Low | Rundown angle below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4513 | Info | Result Final Torque High | Final step torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4514 | Info | Result Final Angle High | Final step angle exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4515 | Info | Result Final Torque Low | Final step torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4516 | Info | Result Final Angle Low | Final step angle below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4517 | Info | Result Tightening Timeout | Tightening time limit exceeded. For General Tightening Strategies max tightening time is 30 seconds. For Multistep max tightening time depends on step restriction Maximum Time Limit. Error code is dependent on tightening stage. | Redo tightening. | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4518 | Info | Result Trigger Lost | Tool trigger was released before target was reached. For General Tightening Strategies it is not allowed to release the trigger before the tightening stage has finished. For Multistep, the error is displayed when trigger is lost before the target in a specific step is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4519 | Info | Premature Torque Loss | Socket has slipped off the nut. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4520 | Info | Result Target Reached Before Final Step | Target torque reached before final step in tightening program. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4521 | Info | Result Post View Torque Low | Post view torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4522 | Info | Result Post View Torque High | Post view torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4523 | Info | Result Post View Torque Interval Not Reached | Post view torque interval not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4524 | Info | Result Torque Compensation Interval Not Reached | Torque compensation interval angle before rundown end not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4525 | Info | Result Tool Movement Exceeded | From a NOK tightening detailed status. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4526 | Info | Result SafetyCurrMon Sensor Mismatch | Current monitoring error. |  |  | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4527 | Info | Result Tool Movement Exceeded |  |  |  | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4538 | Info | Result Final Supervision Torque Low | Final Supervision Torque was not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4543 | Info | Result Snug Monitor High | Wrench only. Monitor detected snug value exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4545 | Info | Result No Residual Torque | Wrench only. Residual torque was under threshold. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4546 | Info | Result Overspeed | Wrench only. Wrench gyro failed to measure angle due to high speed. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4547 | Info | Result Effective Loosening | Wrench only. Wrench detected unexpected loosening. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4548 | Info | Result Final Less Than Target | Final torque is below target torque set in tightening program. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4549 | Info | TurboTight Time Limit Exceeded |  |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4550 | Info | Result Rundown Pulses High | Maximum number of rundown pulses is exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4551 | Info | Result Rundown Pulses Low | Rundown is completed before the minimum number of rundown pulses is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4552 | Info | Result Final Pulses High | Maximum number of pulses is exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4553 | Info | Result Final Pulses Low | Tightening is completed before the minimum number of pulses is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4554 | Info | Current At Shutoff High | Current at shut off exceeded Current Limit High. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4555 | Info | Current At Shutoff Low | Shut off current measured was below Current Limit Low. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4556 | Info | Uncategorized Multistep Error | An error in the multistep configuration, often with tool validation. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4557 | Info | Result Overload |  |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Tightening Process
4600 | Warning | Data Drop or Data Hold used in combination with Batch Tightening. The signals have no effect |  | Data Drop and Data Hold are only supported for worktasks, without batch control. Select another worktask if the signals must be used. |  | Flex StepSync | Tightening Process
4601 | Info | Data Hold Active: tightening result is sent once signal is low |  |  |  | Flex StepSync | Tightening Process
4602 | Info | Data Drop active: tightening result discarded |  |  |  | Flex StepSync | Tightening Process
5010 | Warning | Invalid Tightening Program Parameter Value | The parameter in the selected tightening program are invalid. | Check the configuration of the selected tightening program to find and to change the value of the parameter. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Program Configuration
5011 | Warning | Couldn't prepare program storage in tool | It is not possible to read the current program storage size in the STB tool, or to prepare the program storage for downloading the updated - or newly selected - tightening program to the STB tool. | Check the STB tool for supported software version. Reboot the STB tool. Select again the tightening program. Check network connection for data consistency and quality. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Program Configuration
5020 | Info | Main Trigger Is Not The Active Start Source | Generated when configured for push start only and user presses main trigger. Will be generated until user presses the push start. | Press push start to start the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Program Configuration
5030 | Info | Tightening Program Complexity Exceeds Tool Capacity | The selected tightening program is too complex for the STB tool that is used. Tool will be locked. | Reduce complexity of the tightening program, or choose different program. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Program Configuration
6010 | Info | Accessory Connected | Accessory is connected to the controller. |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6020 | Info | Accessory Disconnected | Accessory is disconnected from the controller. |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6021 | Warning | Fieldbus Offline | No communication with Fieldbus. |  | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6030 | Warning | Accessory Address Collision | Two or more accessories with the same address are connected. | Change address on accessory. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6040 | Warning | Accessory Communication Error | Intermittent communication error with accessory. | Check cables and connectors. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Accessory
6041 | Warning | Fieldbus Error | Communication error with Fieldbus. |  | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Accessory
6042 | Warning | Fieldbus Module Mismatch | The installed Fieldbus module does not match with the configured module. | Change the configuration to match with the installed module, or replace the installed module with the correct one. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Accessory
6043 | Warning | Fieldbus Output Buffer Overflow | The output buffer used for the Fieldbus communication is exhausted and an overflow of the buffer has occurred. One or more signal updates have been discarded. | Stop Fieldbus communication and Fieldbus diagnostics (if used) to recover the buffer. If this event occurs frequently, check your Fieldbus communication setup, including the PLC program: too frequent updates compared to your update interval can lead to this scenario. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync | Accessory
6044 | Warning | Fieldbus Provider ID mismatch | The installed fieldbus module is not supported. | Connect a supported Atlas Copco fieldbus module. | Log Display Ack | Power Focus 8 | Accessory
6050 | Info | Wrong Socket Selected | Generated when no or incorrect socket is selected. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Accessory
6090 | Warning | Barcode Scanner Could Not Be Identified | When no unique serial number is found. | Configure the barcode reader device. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Accessory
7010 | Info | Message Text To Display | General event for displaying of messages. |  | Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC PFHC | Message
8200 | Info | Failed To Open Serial Port | Serial port to be used could not be opened. | Check serial port connections. | Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Miscellaneous
8300 | Warning | Open Protocol client communication timed out | Communication to an Open Protocol client has timed out. No keep alive message or command sent within expected time. | Check controller network connection. Check network setup: firewall and switches. Check client side application software. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 StepSync Power Focus XC | Miscellaneous
8214 | Error | EHMI Software Version Mismatch | EHMI software version does not match in compatibility with the controller. | Update the software version of the EHMI. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Miscellaneous

## Glossary

Conf - Event Codes list

Tells the user whether it is possible to configure the event through the "Configure Event" page.

Available for - Event Codes list

List of products for which the event code is available.

Groups - Event Codes list

Group which the event codes belong to.

Event Description

A short description of the event and why it occurs.

Procedure - Event Codes list

If applicable, the procedure contains an instruction on how to clear the event.

Log - Event Codes list

Tells the user whether the event is to be saved in the event log or not. The value in this list is the default value.

display - Event Codes list

Tells the user whether the event is to be displayed on the screen or not. The value in this list is the default value.

Ack - Event Codes list

Tells the user whether the event must be acknowledged or not before you can proceed. The value in this list is the default value.

Event code

The unique event number.

Type of events - Event Codes list

Type of event: Info, Warning, and Error.

Event name

A descriptive name of the event.