# Configuration of the Dual Transducers

Available for FlexSystem and StepSync.

Dual transducer | Description
--- | ---
Required dual torque | If the connected tool must have dual torque transducers (that are not disabled) to be able to run a tightening.
Required dual angle | If the connected tool must have dual angle transducers (that are not disabled) to be able to run a tightening.
Secondary torque in trace | If the values from the secondary torque transducer is included in the trace.
Secondary angle in trace | If the values from the secondary angle transducer is included in the trace.
Enable double torque restriction | If the double torque transducer restriction is active.
Maximum torque difference | The limit for the double torque difference restriction.
Enable double angle restriction | If the double angle transducer restriction is active.
Maximum angle difference | The limit for the double angle difference restriction.