# Specifying settings for manual station

You must first navigate to Smart AMS Config.

Manual stations are not controlled by Smart AMS.

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: https://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

- To switch to the Workplaces section, select in the Navigation Panel on the left of the page.

- Select the icon of the manual station.

Active toggle switch: If this toggle switch is turned off, the station is inactive. The icons of inactive stations appear hatched. Inactive stations are ignored. If turned on, the station is activated.

Station name field: Specify the name of the station.

Station number field: Specify the ordinal position of the station in the assembly line. Examples: 1, 2, 3.

Description (English) field: Provide a description for the station in English.

Description (local) field: Provide a description for the station in your local language.

## Applies to: