# STRwrench EV Cover Controller Advanced 80 Nm

## Attachments

# Declarations

# Regional Requirements

WARNING

This product can expose you to chemicals including lead, which is known to the State of California to cause cancer and birth defects or other reproductive harm. For more information go to

https://www.p65warnings.ca.gov/

# Safety

DO NOT DISCARD - GIVE TO USER

WARNING

Read all safety warnings, instructions, illustrations and specifications provided with this power tool.

Failure to follow all instructions listed below may result in electric shock, fire, and/or serious injury.

Save all warnings and instructions for future reference.

WARNING

All locally legislated safety rules regarding installation, operation and maintenance shall be respected at all times.

## Statement of Use

- For professional use only.

- This product and its accessories must not be modified in any way.

- Do not use this product if it has been damaged.

- If the product data or hazard warning signs on the product cease to be legible or become detached, replace without delay.

- The product must only be installed, operated and serviced by qualified personnel in an industrial environment.

In this Section

- Intended use
- Safety Signal Words
- Product Specific Instructions

# Intended use

This product is intended for use on or in close proximity to energized electrical apparatus or conductors operating at maximum voltage of 1000 V.

# Safety Signal Words

The safety signal words Danger, Warning, Caution, and Notice have the following meanings:

DANGER | DANGER indicates a hazardous situation which, if not avoided, will result in death or serious injury.
WARNING | WARNING indicates a hazardous situation which, if not avoided, could result in death or serious injury.
CAUTION | CAUTION, used with the safety alert symbol, indicates a hazardous situation which, if not avoided, could result in minor or moderate injury.
NOTICE | NOTICE is used to address practices not related to personal injury.

# Product Specific Instructions

# Installation

# General Installation Safety

WARNING

High Voltage Hazard

Insulated tool covers must always be used together with isolated sockets.

- Do not use insulated tool covers without isolated sockets.

- Install the insulated tool covers securely, always follow the installation instructions.

- Replace the insulated tool covers if they are damaged in any way.

# Installing the EV Cover

When the insulated cover is installed, the shock indicator is not visible.

1. Attach the two halves of the LED ring protection to the two halves of the EV cover as follows:

   - Attach the half of the LED ring protection that has a beveled positioning pin with the positioning pin facing the front of the EV cover.

   - Attach the half of the LED ring protection that has a square positioning pin with the positioning pin facing the back of the EV cover.

2. Attach the two halves of the EV cover to the STRwrench by inserting the eject pin into its spot.

3. Gently press and remove the button cover on the insulated frame for the STRwrench display. Then, place the button cover on the STRwrench button, and attach the insulated frame to the STRwrench display.

4. Insert the rubber profile on the insulated display frame.

5. Insert the four rubber rings on the EV cover.

6. Attach the label with the following information: tool capacity, controller serial number, smartHEAD S/N.

# Removing the EV cover

Do not remove the EV cover from the tool until you must remove it for tool servicing.

1. Remove the four rubber rings from the EV cover.

2. Remove the rubber profile from the insulated display frame.

3. Remove the insulated frame and the insulated button cover from the display.

4. Separate and remove the two halves of the EV cover and the eject pin from the STRwrench.

# Operation

# General Operation Safety

WARNING

High Voltage Hazard

Accidental contact with any high voltage may result in severe injury or death.

- Always use insulated tool covers together with isolated sockets.

- Do not use insulated tool covers if they are damaged in any way or if they are not correctly installed.

- Only the parts of the tool covered by insulated tool covers are protected against high voltage. The other parts of the tool are not protected against high voltage.

## Inspection Before Use

- Visually inspect this product every time before use.

- If there is any doubt concerning the safety of this product, a suitably trained person must examine it and retest it, if necessary.

## Temperature

- Use this product in an industrial environment with a regulated temperature.

- Do not use this product in temperatures above 40°C or in high atmospheric humidity.

# Service and Maintenance

# General Service and Maintenance Safety

## Storage

- Store this product properly so as to minimize the risk of damage to the insulation due to storage or transportation.

- Store this product separated from other tools to avoid mechanical damage or confusion.

- Protect this product from excessive heat as well as from UV radiation.

## Periodic Examination

A suitably trained person should perform an annual visual examination of this product to determine its suitability for further service.

# Information on Environmental Labeling of Packaging

Material | Abbreviation | Numbering
--- | --- | ---
High density polyethylene | HDPE | 2
Polyvinyl chloride | PVC | 3
Low density polyethylene | LDPE | 4
Polypropylene | PP | 5
Polystyrene | PS | 6
Polyurethane | PU | 7
Corrugated fibreboard | PAP | 20
Non-corrugated fibreboard | PAP | 21
Paper | PAP | 22
Wood | FOR | 50
Paper and fibreboard/plastic | C/PAP | 81

EU Decision 129/97/EC.

# Signs and Stickers

The product is fitted with signs and stickers containing important information about personal safety and product maintenance. The signs and stickers shall always be easy to read. New signs and stickers can be ordered by using the spare parts list.