# Interconnecting Multiple Controllers with an E-stop

WARNING

Risk of Severe Injury or Death

The emergency stop will not operate correctly if an incorrect type of e-stop cable is being used. This may result in severe injury or death.

- Make sure that the product number of the e-stop cable that is being used, matches the product number in the instruction.

WARNING

Risk of Severe Injury or Death

The emergency stop will not operate correctly if the e-stop cables are connected incorrectly. This may result in severe injury or death.

- Make sure that each specific cable connector is connected to the correct port.

If using E-stop cable 1m Special or E-stop cable 3m Special, the following steps must be applied:

When interconnecting multiple controllers with an e-stop, e-stop cables labeled Master side and Member side must be used. The connector next to the label with the text Master side, must always be connected to the E-STOP OUT port on the controller. The connector next to the label with the text Member side, must always be connected to the E-STOP IN port on the controller.

## Applies to: