# Compatibility Matrixes

The controller type and the generation of the controller determines which e-stop cable that must be used. Refer to the compatibility matrixes below to know which e-stop cable to use.

The synchronized tightening system will not function if controllers from both matrixes below are used in the same synchronized tightening system. Use only controllers and cables from one of the two matrixes below when setting up a synchronized tightening system.

Matrix 1
Controller type | Controller product number | Controller generation | E-stop cable product number
--- | --- | --- | ---
PF8 | 8436280002 | A, B, C | 4220903401 4220903403
PF8 LV | 8436281002 | A, B, C
PF8 HV | 8436282002 | A
PFS | 8436280003 | A
PFS HV | 8436282003 | A

Matrix 1: Any combination of the controllers in Matrix 1 can be used in one synchronized tightening system.

Matrix 2
Controller type | Controller product number | Controller generation | E-stop cable product number
--- | --- | --- | ---
PF8 | 8436280002 | D | 4220880001 4220880003 4220880005
PF8 LV | 8436281002 | D
PF8 HV | 8436282002 | B
PFS | 8436280003 | B
PFS HV | 8436282003 | B

Matrix 2: Any combination of the controllers in Matrix 2 can be used in one synchronized tightening system.

## Applies to: