# Service Recommendations

- On return from each job and before allocation for later work, examine the completeness of the ACMS08T or ACHS14T kit. Also examine the items to make sure that they are serviceable.

- Replace any missing or damaged items as soon as possible and before using the tool again.

- Store the ACMS08T and ACHS14T in a cool dry place and make sure that all machined surfaces are greased.

- Grease all moving parts before use.

## Applies to: