# Configuring ILM Protocol

Most configuration fields are not supported anymore, even though they are still visible in PX2 3.10 and 3.11. Below are the valid configuration fields.

1. Select Virtual Station.

   For IxB, navigate to Integrated Controller Tool.

2. In the Virtual Station tab, select ILM Protocol.

3. Select ON.

4. Configure the port number of the ILM Protocol adapter if needed. The default port number is 13141 and is shared by all Virtual Stations in the controller.

   This step is not applicable for integrated controller tools.

5. Enter the ILM Tag ID used for the Virtual Station.

   This step is not applicable for integrated controller tools.

6. In Locking permitted, select On if you want the tool be locked by ILM.

   When turned On the tool will be locked outside the enable area by ILM Protocol.

7. In Log level, Choose the level of detail of the logs.

   Analysis of Communication : This is a mode for the developers (not recommended for the customer).

   Error messages : Only the most necessary error messages are logged without further context.

   Information : Error messages and the basic context are logged.

   Debug : Maximum level of detail, this should only be set on request.

   The logs are included when exporting All information, under Export/Import in the Virtual Station.

8. In ILM Manager, make sure that the ILM Tag is configured to use ILM Protocol. See the Configuring Controller Communication chapter in the ILM Manager User Guide.

For connection status, see Viewing ILM Protocol Status.