# Activating a License

During this operation, the connection between the device and the STRwrench QA Inspector Software web user interface must be via USB cable.

1. Connect the STRwrench to the computer via USB cable.

2. Access the STRwrench QA Inspector Software web user interface.

3. On the web user interface sidebar menu, select Integrated Controller Tool .

4. On the Integrated Controller Tool page, select the Licenses tab.

5. In the upper-right corner of the Licenses tab, click Add.

6. Under Step 1 - Generate Capability Request, enter in the dedicated field the activation code you have been given. Then, click Generate to download the Capability Request file.

7. Go to the License Activation Portal at https://atlascopco.flexnetoperations.com and upload the Capability Request file to download the Capability Response file.

8. Under Step 3 - Upload the Capability Response, click Choose file to browse and upload the Capability Response file.

The activated license is displayed in the Licenses list with Status set as Active.

Relevant Information

- Accessing the Web User Interface