# Configuring the ToolsNet Connection

1. On the home menu, tap Configuration > External systems > ToolsNet.

2. On the General tab, select Enabled.

3. On the PIM tab, enter the following parameters:

   Parameter | Description
   --- | ---
   Address | Enter ToolsNet server IP address.
   Port | Enter ToolsNet server port. Range value: 1 - 65535; default value: 9014.

4. On the Configuration tab, enter the following parameters:

   Parameter | Description
   --- | ---
   Station number | Enter the number that ToolsNet must associate to the results collected by STRwrench. Range value: 1 - 9999.
   Station name | Enter the name that identifies STRwrench in ToolsNet tree structure.
   Send traces | Select the checkbox to enable STRwrench to send traces to ToolsNet

5. On the top bar, tap Apply .

For further information on how to use ToolsNet 8, refer to ToolsNet 8 User Guide.