# Editing a Joint Inspection

1. On the home menu, tap Joints.

2. On the Joints page, tap the row of the joint linked to the inspection to edit.

3. In the Inspections category of the Edit joint page, tap the row of the inspection to edit.

4. On the Edit inspection page, edit the required inspection parameters in each category.

5. On the top bar of the Edit inspection page, tap Apply .

Relevant Information

- Cp/Cpk Inspection Parameters
- SPC Inspection Parameters